11/19/2021 - Build 284
	- Current full version is 4.3.284 (CD version must be 4.3)
	- Boost.LAN now use .net framework version 4.5
	- Fix BSOD on multiprocessor running multiport data transfer failed due to DPC and SpinLock issue.
	- Fix Connection Check and space check timer issue BSOD now fixed.
	- ExSetTimerResolution causing BSOD is now fixed and removed that API.
	- Synchronization issue fixes.
	- Firmware upgrade progress messages are now descriptive and informative.
	- Firmware upgrade issue due to VSLM Mask is now fixed.
	- Boost.LAN now use .net framework version 4.5
17/05/2017 - Build 250
	- DEBUG: Development test build for BSOD investigation.
26/04/2017 - Build 249
	- ADD: Wait for passive level execution to finish when disconnect.
	- UPDATE: sign code signing certificate update
	- FIX: High Perfomrance issue with 2 stopbits (or Seiki app)
30/03/2017 - Build 248
	- DEBUG: BSOD issue, now unregister read callback on disconnect
	- DEBUG: BSOD issue due to read (passive level execution process) still going on after close
28/02/2017 - Build 247
	- FIX: BSOD due to data coming after port close.
	- CHANGE: copyrights year now set to 2017
23/02/2017 - Build 246
	- FIX: TELNET_SE parsing causing notifcation packet to drop.
17/02/2017 - Build 245
	- FIX: DCD toggle issue causing data transfer to stop or not start transmitting.
	- DEBUG: getting extra modem status request
09/09/2016 - Build 244
	- Change CD version to 3.7
21/06/2016 - Build 243
	- FIX/ADD: Tiva upgrade issue on f/w upgrader.
23/09/2015 - Build 242
	- Fix for Advanced Connection Validation issue, when in RAW TCP mode, can't force COM port to connect in RFC2217 mode.
10/09/2015 - Build 241
	- VCP driver BSOD in CAT test due to invalid pointer access.
02/09/2015 - Build 240
	- Connection check timer recursive call causing BSOD is now fixed.
18/08/2015 - Build 239
	- More Half Duplex mode fix and code error.
13/08/2015 - Build 238
	- Half Duplex test failed fixes.
13/08/2015 - Build 237
	- Build for debugging
11/08/2015 - Build 236
	- Build for debugging
29/07/2015 - Build 235
	- Introduce Write request delay in driver for classic mode wrtie are disable by default.
	- 2nd Port Duplex mode gets overwritten in f/w due to Driver setting is now fixed.
15/07/2015 - Build 234
	- Introduce Write request delay in driver for classic mode wrtie.
29/06/2015 - Build 233
	- Fix for Seiki BSOD on ExSetTimerResolution due to API get executed on DISPATCH Level.
24/03/2015 - Build 226
	- Fix throughput issue with high baud rate transmit.
19/03/2015 - Build 225
	- Fix Predator software issue.
10/03/2015 - Build 224
	- Added ES-413, ES-420, ES-401 and ES-479 devices.	
21/01/2015 - Build 221
	- Added ES-426 and ES-457 devices.
	- Fix multiple device port forwarding issues.
03/07/2013 - Build 211
	- Added support for Windows 8
	- Fix Uninstall application required legacy command which required NTVDM enabled
	- Low Baud Rate issue where the emulation count is incorrect, and data in FIFO get flushed too early before all of them are transmitted successfully
	- Fixed: Written length information of Write request while write timeout occurred is incorrect.
	- Allen-Bradley PanelView PLC communication (SERIAL_XOFF_COUNTER issue)
	- Low baudrate issue in emulation of trigger levels
	- Maximum Baud Rate changed from 921600 to 1000000
	- Null stripping BSOD fix.
	- fixed SERIAL_PURGE_TXCLEAR flag issue in VCP and now it sent to ES device when purge is called.
	- Xon/Xoff stripping issue fix.
	- Fixes 64 bit issues.
	- Port close issue in low baud rate fix
Version 3.0.195.0 - 12/12/2012
- Bug fix for Control Queue freezing PC issue. (ES0886_ES-522_FW4.16_Build187_Replace)
- Bug fix for Suite Upgrade
- Bug fix for Driver Update in 64bit OS

Version 3.0.191.0 - 29/11/2012
- Bug fix for E2S_WIN_FUN_007_REPLACE test failed. (ES0886_ES-522_FW4.16_Build187_Replace)
- Bug fix for Import Export doesn't work for port mode and override (ES8078_ES-522_FW4.13_Build184_Import Export doesn’t work for Port Mode)
- Add feature that will copy product manuals (ES0890_ES-511_FW4.17_Build187_Product Manual in Boost.LAN)
- Bug fix for when proxy is on, find device need to click more than once (ES8079_ES-522_FW4.13_Build184_ProxySever doesn’t work properyl)
- IRP_MJ_FLUSH_BUFFERS is implemented (ES0868_Build174_Fw4.07_CloseApp at high baudrate fails)
- Bug fix for UI is not updating properly when device is disable/enable from devicemanager (ES0799_ES-279_FW3.28_Build145_Boost.LAN shows doesn’t update device from disable correctly)

Version 3.0.188.0 - 13/11/2012
 - Bug fix for RXOVER due to screen saver issue. (ES0885_ES-522_FW4.16_Build187_Soak test)
 - Bug fix for HD soak test can't kick start. (ES0889_ES-522_FW4.17_Build187_Half duplex soak test)
 - Bug fix for device property page is not working. (ES8084_ES-511_FW4.15_Build185 Some tool tips not working)
 - Fix for support page link is broken (ES8083_ES-511_FW4.15_Build185 Property page help doesn’t link to right page)
 - Fix for ES-101 COM Port installtion issue (ES0864_ES-101_FW4.06_Build173_COM Port installation)
 - 
Version 3.0.187.0 - 31/10/2012
 - Bug fix for ES Industrial range device 422/485 mode is not changed during installation. 
 - Bug fix for Win7 64 bit issue with applying Bus driver related settings.
 - Implement 1.5 stopbits range for 4&8 port and industrial range.
 - Connection Attempt timeout implemented.
Version 3.0.178.0 - 05/10/2012
 - Bug fix for TCP/IP device property page resotre default causing registry corruption in Build 177.
Version 3.0.177.0 - 01/10/2012
 - Bug fix for device property page data do not saved properly in Build 176.
Version 3.0.176.0 - 17/09/2012
 - Bug fix for low baud rate data written notification causing issue when sendind double 0xFF and counting statistic causing write to timeout.
Version 3.0.175.0 - 17/09/2012
 - Add support for ES-125.
Version 3.0.174.0 - 13/09/2012
 - Fix uninstallation issue with ES-522.
Version 3.0.173.0 - 31/08/2012
- Fix issue of DDK's User Interface class issue when device property page load up the web configuration page causing port disabled.
Version 3.0.172.0 - 14/08/2012
- Fix issue of finding devices from different subnet while plug-in at the same media (same physical LAN)
- Fix application load up delay.
- Add support for ES-125.
Version 3.0.171.0 - 07/08/2012
- Add support for ES-511, ES-522, ES-551, ES-571, ES-031, ES-042
- Device property page's override settings are not obsolete and user can change override settings only from the device's web page.
- RS-422/485 Duplex mode can also be change from device's web page only and Duplex setting tab is removed from the advanced setting dialog box.
Version 3.0.170.0 - 11/06/2012
- Fix for when using redirection pipe to COM port in command line with low baud rate, the last bytes are cut off.
Version 3.0.169.0 - 24/05/2012
- Fix for, when "Port Accessible When Device is Offline" tick box is ticked from device property page and open the port, handshake line RTS and DTR are not properly set.
