03/11/2020 - Build 132
	- Change CD version from 5.0 to 5.1

02/11/2020 - Build 131
	- Fix US-159 COM no flow control error
	- WPP tracing issue

26/10/2020 - Build 130
	- US-70102 COM assignment is now set to 4/5/6/7
	- Fix service issue for US-159 installation

21/10/2020 - Build 129
	- 2nd Device plug in COM assingnment issue fixed

05/10/2020 - Build 128
	- Co-Installer doesn't assign COM port in sequence as needed for US-70102

03/10/2020 - Build 127
	- COM Number assigment was not working properly

29/09/2020 - Build 126
	- Update with latest Windows DDK
	- Driver package support starting from Windows 7 and upwards
	- Update driver projects to VS2019
	- Add support for US-70102

26/01/2015 - Build 110
	- Fixed divided by zero BSOD for Windows 7
	- Change low baud rate emulation speed to start from 57600 and below
	- Fix the high data transmission gap issue for Cummins
09/05/2014 - Build 107
	- Added Windows 8.1 support
	- Fix support hyper link under uninstallation programs list
	- Fix Uninstall application required legacy command which required NTVDM enabled
	- Low Baud Rate issue where the emulation count is incorrect, and data in FIFO get flushed too early before all of them are transmitted successfully
	- Added support for US-235, US-320, US-159, US-010, US-376, US-030 products
01/08/2013 - Build 100
	- Ignore hardware serial number for VX-02301 so that any device plugged in would have the same settings, COM89 with HalfDuplex. Fixed in hardware where the VX-02301 is programmed with the same unique serial number. Nothing has changed in drivers.
	- Addes new product description in INF file for VX-02301 product
29/07/2013 - Build 98
	- Added support for VX-02301 which default to COM89 for Cummins.
03/06/2013 - Build 97
	- Fixed: Written length information of Write request while write timeout occurred is incorrect.
02/05/2013 - Build 96
	- Allen-Bradley PanelView PLC communication (SERIAL_XOFF_COUNTER issue)
	- Low baudrate issue in emulation of trigger levels
	- Maximum Baud Rate changed from 921600 to 1000000
	- Add EDref PnP ID into INF File
30/01/2013 - Build 94
	- Santander device US-25701 Support. Install with default COM2 and COM4.
05/10/2012 - Build 91
	- Windows 8 Support
	- Unicode Support
14/04/2011 - Build 84
	- Null stripping BSOD fix.
08/06/2010 - Build 83
	- Upgrade COM label issue on build 82
25/05/2010 - Build 82
	- fix on Purge delay.
	- Set default Maximum Latency to 2ms, for cummins
18/12/2009 - Build 81
	- fixed SERIAL_PURGE_TXCLEAR flag issue in VCP and now it sent to ES device when purge is called.
3/12/2009 - Build 80
	- Xon/Xoff stripping issue fix.
1/12/2009 - Build 79
	- Fixes 64 bit issues.
1/10/2009 - Build 76
	- Port close issue in low baud rate fix
29/9/2009 - Build 75
	- Bug fixes for the test
	- Fixe for device scan Windows 7 test.
30/7/2009 - Build 73
29/7/2009 - Build 72
	- Vista 32 "Plug and Play Driver DTM Test" fix
	- USB transaction error issue fixed.
	- typo error in inf file.
15/7/2009 - Build 71
	- XonXoff issue updated.
3/7/2009 - Build 70
	-  4 port and 8 port uninstallation issue that remove the MS hub driver.
19/6/2009 - Build 69
	-  Remove multiple entries of revision for US-101, US-324, US-357, US-257, US-313, US-701, US-346, US-279, US-824, US-160 in inf files and setup program.
	-  Port upgrade issue
07/04/2009 - Build 66
	- Added support for US-101, US-324, US-357, US-257, US-313, US-701, US-346, US-279, US-824, US-160 in inf files and setup program.
	- Added 9 different revision of PnP ID for above cards
	- Rename Boost.USB to Boost
12/09/2008 - Build 64
	- Fix for Xon/Xoff Limit size > 16K
	- fix for data corruption during baud rate change.
04/06/2008 - Build 63
02/06/2008 - Build 62
	- VX-034 installtion issue with 64-bit OS
	- Fix for file transfer issue with HyperTerminal.
25/04/2008 - Build 61
18/04/2008 - Build 60
15/04/2008 - Build 59
	- add Tx Fifo emulation functionality.
10/04/2008 - Build 57
	- fix the device property page can't set Space parity settings.
08/04/2008 - Build 56
02/04/2008 - Build 55
	- Bug fixes RxOver at 921600 on Xon/Xoff.
	- Add US-606, US-400, US-800 and US-160 id.
26/03/2008 - Build 53
	- Bug fixes USB read stop intermittently during data transfer at multiprocessor pc.
7/03/2008 - Build 50
	- Bug fixes issue Build 49.
21/02/2008 - Build 48
	- Bug fixes Uninstall issue with Build 47.
15/02/2008 - Build 47
	- Bug fixes Uninstall issue with Build 46.	- 
13/02/2008 - Build 46
	- Bug fixes for data loss after power mode on Xon/Xoff handshaking.
	- Fix Xon/Xoff character processing on port driver.
11/02/2008 - Build 45
	- Bug fixes from Build 44
31/01/2008 - Build 44
	- Bug fixes from Usb2Serial2 FTC1
29/01/2008 - Build 43
	- Bug fixes from Usb2Serial2 FTC1
	- half duplex test failed fixes.
25/01/2008 - Build 42
	- Bug fixes from bug list.
	- fix DTA didn't recognized the 422/485 port.
	- WMI & Perfmon counter added.
23/01/2008 - Build 41
	- 422/485 Device property page bug fixes.
	- Upgrade device fixes. (Note: only allow card upgrade from this version.)
18/01/2008 - Build 40
	- Fix: Bug fixes from USB2Serial1.
	- Upgrading port will show warning message.
15/01/2008 - Build 39
	- Fix: Fix RTS signal for 422/485 card.
10/12/2007 - Build 38
	- Fix: WPP traceing buffer overrun error.
07/12/2007 - Build 37
	- Fix: Memory acess error while processing Xon/Xoff Character.
30/11/2007 - Build 36
	- Fix: Jumpy Mouse issue
	- Fix: port registry persistant.
30/11/2007 - Build 35
	- Fix: Upgrade issue on both port and Card driver
27/11/2007 - Build 34
	- Fix: Uninstallation during port open
	- fix: soak test data loss
21/11/2007 - Build 32
	- Fix: Data overrun issue when CPU is 100% busy
15/11/2007 - Build 31
	- Fix: Latency not set after first time port opening.
09/11/2007 - Build 30
08/11/2007 - Build 29
07/11/2007 - Build 28
	- Build for FTC2. 
06/11/2007 - Build 27
05/11/2007 - Build 26
	- Bug fixes for TC7.
23/10/2007 - Build 23
	- Xon/Xoff test fixes.
15/10/2007 - Build 22
15/10/2007 - Build 21
	- Bug fixes for Full Test Cycle 1. See bug list for more info.
04/10/2007 - Build 20
	- Fix for Baud 680000 error.
	- Fix Data bits entry error in Device property page.
